





Adding wire less security




















Enable isp router to assign public ip

First configure IP addresses and a DHCP server on ISP router.









Now make the internet interface a DHCP client by enabling DHCP on it.

